| > Home > How To # Timeout You can set the length of time before a timeout occurs. An error occurs if this time is exceeded. If you set larger values, it takes more time to search for the network interfaces. Select Refresh from the Display menu or restart EpsonNet Config to activate the settings.
Item | Explanation
Time before comm. error when acquiring information (2-900) | Set the length of time before a timeout occurs (between 2 and 900 seconds). The default value is 25 seconds.
Time before comm. error when setting information (2-900) | Set the length of time before a timeout occurs (between 2 and 900 seconds). The default value is 25 seconds.
Time to wait before rebooting (60-900) | Set the length of time before a timeout occurs (between 60 and 900 seconds). The default value is 300 seconds.
Restore to default settings button | Reverts the network interface to the factory default settings.
OK button | Saves the settings.
Cancel button | Cancels any changes.