| > Home > How To # Registering FAX Numbers Editing the FAX Number Individually Batch Registration of FAX Numbers ## Editing the FAX Number Individually
| Select the target network interface.
| Click the Configuration button.
| Click Fax Number under Fax.
| Select the number you want to edit, then click Edit.
| Edit the items, then click OK.
| Click the Transmit button.
Top ## Batch Registration of FAX Numbers ### Creating the setting file
| Select the network interface you want to configure.
| Click the Configuration button.
| Click Fax Number under Fax.
| Click the Export button.
| Enter the file name, then click Save.
| Open the file in the spreadsheet software, then edit the information.
| Save the file as SYLK file (*.slk).
### Making the Batch Settings by Importing the Setting File
| Select the network interface you want to configure.
| Click the Configuration button.
| Click Fax Number under Fax.
| Click the Import button.
| Click OK.
| Click Browse, then select the SYLK file (*.slk) containing the fax number information, then click Open.
| Click Next.
| Click OK.
| Click the Transmit button.
Note:
If the setting file contains errors, the error screen is displayed. Confirm the setting file.
Top |